For 1990-2009 cars

Checks | Causes
--- | ---
Centre Support with 2-6 Low and Reverse Clutch Assembly (67) |

• | Inspect for damaged or worn low and reverse clutch plates (463-465).

• | Inspect for damaged low and reverse clutch backing plate (462). Inspect for worn splines on backing plate.

• | Inspect for damaged low and reverse clutch backing plate retaining ring (461).

• | Inspect for damaged low and reverse clutch piston assembly (470), spring (469), spring retaining ring (466), and centre support assembly (459).

• | Inspect for damaged low clutch sprag assembly (467). Holding the sprag assembly with the retaining ring facing up, and the inner race of the sprag assembly fixed, the outer race should freewheel counterclockwise.

• | Inspect for cut, worn, or damaged low clutch sprag seal (468).

Output Carrier Assembly (68) | Inspect for damaged or stripped splines on the output carrier assembly.