For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Connect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Insert a suitable tool under the puddle lamp housing (1) and release the locking tab (2) of the lamp.
3. Pry the lamp assembly from the mirror and pivot and lower the assembly.
4. Bend back the lever contact that holds the bulb and remove the bulb from the lamp housing.

### Installation Procedure

1. Install the new bulb to the puddle lamp assembly.
2. Feed the lamp wiring into the cavity and push the lamp back into the door mirror housing.
3. Connect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection.
4. Check all vehicle lights for correct operation.