For 1990-2009 cars

### Removal Procedure

1. Fully extend the head restraint (2) out of the head restraint guides (1).
2. Insert a suitable size probe into the hole in the restraint guide (4).
3. Depress the head restraint sleeve height adjuster lock (2).
4. With the aid of an assistant remove the head restraint (1) from the seat assembly (3).

### Installation Procedure

1. Locate the head restraint (2) in the head restraint guides (1).

Important: Listen for an audible click to confirm fitting.

2. Install the head restraint (2) by pushing downwards into the head restraint guides (1).