For 1990-2009 cars

### Removal Procedure

1. Remove the knee bolster. Refer to Knee Bolster Replacement .
2. Remove the right close out panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side .
3. Remove the hood release handle. Refer to Hood Primary Latch Release Cable Replacement .

Important: The right side is shown, the left side is similar.

4. Remove the I/P retainer to I/P carrier retaining screws (1).
5. Remove the I/P retainer.

### Installation Procedure

1. Align the I/P retainer to the I/P carrier.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the I/P retainer to I/P carrier retaining screws (1).

Tighten
Tighten the screws (1) to 2 N·m (18 lb in).

3. Install the hood release handle. Refer to Hood Primary Latch Release Cable Replacement .
4. Install the right close out panel. Refer to Instrument Panel Insulator Panel Replacement - Right Side .
5. Install the knee bolster. Refer to Knee Bolster Replacement .