For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to General Repair Instructions in the Preface section. Notice: Refer to General Repair Instructions in the Preface section.

#### Preliminary Procedures

1. Thoroughly clean the transmission case assembly, including case threads, with clean solvent.
2. Clean gasket sealing surfaces. Remove all residual gasket material.
3. Inspect all threaded holes. If necessary, repair any thread damage.

1 | Front Case Sealing Surface
2 | Manual Shift Shaft Seal Tip Refer to Manual Shift Shaft Seal Replacement.
3 | Center Support Fluid Passage Seal Bores
4 | Fluid Pan Sealing Surface
5 | Output Shaft Bushing
6 | Rear Case Sealing Surface
7 | Fill Tube Bore
8 | Electrical Connector Passage Sleeve Bore