For 1990-2009 cars

Parameter | Operating Conditions | Expected Value | Definition
--- | --- | --- | ---
Ignition is ON, engine OFF, and vehicle is stationary
Antenna | -- | Main |
Audio Source | CD Mode Selected | CD | This parameter determines which mode the Infotainment is currently using.
Tuner Mode Selected | Tuner
Audio System | System On | On | This parameter determines if the Audio System is On or Off.
System Off | Off
Auxiliary Input | External Device Connected | Active | This parameter displays if their is an external device connected to the Infotainment unit.
External Device Not Connected | Inactive
Balance | Left 1 to 6 | User Dependent | This parameter displays the current balance of the speaker on the left or right sides.
Right 1 to 6 | User Dependent
Band | FM 1 | FM 1 | This parameter displays the currently selected Band.
FM 2 | FM 2
FM ASM | FM ASM
AM | AM
AM ASM | AM ASM
Bass | STD | User Dependent | This parameter displays the current bass setting based off the user's selection.
+1 to +6 | User Dependent
Battery Voltage | -- | 12 Volts | The scan tool displays 0-14 Volts. The scan tool displays approximately 12 Volts when the ignition is On.
Beeps | Beeps activated | On | This parameter displays if the audio unit will beep when buttons are pressed.
Beeps deactivated | Off
Brightness | STD | User Dependent | This parameter displays the currently selected brightness based off the users selection.
-5 to +5 | User Dependent
CD Error | Problem with Unit | Yes | This parameter displays if there is a current error with the audio unit.
No Problem with Unit | No
CD Player Status | Pause button pressed while CD paused | Play | This parameter displays the status of the CD Player.
Pause button pressed while CD playing | Pause
Audio system turned off or change of audio source | Stop
Track up button pressed | Track Up
Track down button pressed | Track Down
Reverse button pressed | Reverse
Cue button pressed | Cue
CD Special Play Mode | Repeat button pressed | Repeat Track | This parameter displays the last CD special play mode that was selected by the user.
Random button pressed | Random Track
Colour | -- | Vehicle Dependent | This parameter displays a numeric value. This number corresponds to the colour of the infotainment unit display.
Contrast | STD | User Dependent | This parameter displays the current contract setting, based off the user's selection.
-5 to +5 | User Dependent
Current CD | -- | Audio CD | This parameter displays the type of disc inserted into the CD Player.
-- | MP3
Current CD Type | CDDA | User Dependent | This parameter displays whether the compact disc is CDDA or MP3.
MP3 | User Dependent
Current Track | 1 to 30 | -- | This parameter displays the current track on the CD been played.
Date | 1 to 31 | -- | This parameter displays the current date stored in the infotainment unit.
Day | Monday - Sunday | -- | This parameter displays the current day of the week stored in the unit.
DDL Bass Attenuation | 0 to 60 dB | User Dependent | This parameter displays the current dynamic distortion bass level.
DDL Setting | Default Setting | Off |
User dependent | Cur 1 to Cur 3
DDL Volume | 0 to 60 dB | 0 dB | This parameter displays the current dynamic distortion volume level.
Dial Turns | Counts | 1 Counts | This parameter displays the numbers of counts the dial has been turned.
Dial Type | Mode dial used | Mode | This parameter displays the last dial type to be used by the user.
Multi-function dial used | Multi-function
Fan speed dial used | Fan Speed
Driver temp dial used | Driver Temp
Display Format | -- | 12 Hour | This parameter displays the time format based on 12 hour or 24 hour format.
-- | 24 Hour
Display Illumination | 1 to 100 % | User Dependent | This parameter displays the current illumination level based from the user's selection.
Drive Type | -- | Single CD | This parameter displays the current drive type as selected by the user
Driver Identification | Programmed Key | Driver 1 | This parameter displays the status of the current ignition key.
Programmed Key | Driver 2
Equalizer | On | User Dependent | This parameter displays if the user has turned On or Off the equalizer settings in the audio unit.
Off | User Dependent
Equalizer Boost | -- | 0 |
Equalizer Preset | -- | On | This parameter displays the current preset for the equalizer.
-- | Off
Fader | STD | User Dependent | This parameter displays the current settings for the fader based off the user's selection.
Front 1 to 6 | User Dependent
Rear 1 to 6 | User Dependent
Fascia Button | Depends on Last button pressed. | -- | This parameter displays the last fascia button pressed during the last ignition cycle.
Field Intensity | -- | 0-300 dBuV | The scan tool displays 0-300 dBuV. The signal from the antenna is measured in dBuV.
Frequency | 87.5 to 108.00 FM | User Dependent | This parameter displays the currently selected radio frequency.
522 to 1710 AM | User Dependent
Hazards | Hazard button pressed | Active | This parameter displays whether the hazard lamps have been activated.
Hazard button depressed | Inactive
Illumination | -- | 0-100% |
Illumination Mode | -- | Auto |
Interior Illumination | -- | 0-100% | This parameter displays the interior illumination as a percentage. The highest percentage will have the interior lamps at their brightest.
Key Stuck | -- | None | This parameter displays if their is currently a button stuck on the fascia plate.
Loudness | Loudness activated | On | This parameter displays if the loudness function has be turned On or Off by the user.
Loudness deactivated | Off
Month | -- | Varies | This parameter displays the current month
Multipath | -- | % |
Multipath | -- | Yes |
-- | No
Mute | Mute button pressed | On | This parameter displays if the audio unit mute button has been activated or deactivated.
Mute button depressed | Off
Navigation Audio Channel | -- | Varies | This parameter displays the audio channel that is utilised for the navigation audio
Navigation | -- | Activated | This parameter displays if the navigation is Activated or Not Activated.
-- | Not Activated
Navigation Volume | -- | dB | This parameter displays the correctly selected volume setting for the navigation system through the audio unit.
Play Time | -- | hh:mm:ss | This parameter displays the play time of the CDDA/MP3.
Preset | 1 to 6 | User Dependent | This parameter displays the currently selected preset radio station.
Rear Aux | Rear aux activated | On | This parameter displays if the rear aux is On or Off
Rear aux deactivated | Off
Rear Controls | Rear controls activated | Active | This parameter displays if the rear seat controls are working correctly.
Rear controls deactivated | Inactive
Search Sensitivity | Local | User Dependent | This parameter displays the currently selected search sensitivity signal strength.
Distant | User Dependent
Auto | User Dependent
Single CD Loaded | CD Loaded into Unit | Yes | The scan tool will display whether their is a compact disc loading or not.
No CD Laded into Unit | No
Speed Dependent Volume | -- | dB | This parameter displays the volume in dB of the infotainment unit dependent on the speed of the vehicle.
Speed Volume Curve | Default Setting | Off | This parameter displays the speed volume curve as defined by the user
User Settings | Cur 1 to Cur 5
Stereo Status | User dependent | Mono | This parameter displays if the audio system on stereo or mono mode based on the user's selection.
User dependent | Stereo
System Power Mode | Ignition is in OFF position | Off | This parameter displays the current ignition cycle the key is on.
Ignition is in ACC position | Accessory
Ignition is in RUN position | Run
Ignition is in CRANK position | Crank
Time | -- | hh:mm:ss | This parameter displays the current time.
Total Track Time | -- | hh:mm:ss | The scan tool will display the total time of the current song.
Treble | STD | User dependent | The scan tool will show the current treble setting as selected by the user.
-6 to +6 | User dependent
Vehicle Speed | -- | km/h | This parameter indicates the vehicle speed calculated by the control module based on an input from the vehicle speed sensor (VSS). The scan tool will display a high value at higher vehicle speeds, and a low value at lower vehicle speeds.
Voice In | Voice in activated | Active |
Voice in deactivated | Inactive
Volume | 0 to 40 | User dependent | The scan tool will show the current user selection.
Year | 2000 to 2099 | -- | The scan tool will show the current year.