For 1990-2009 cars

### Removal Procedure

1. Remove the front door trim panel. Refer to Front Side Door Trim Panel Replacement.
2. Remove the speaker assembly to door frame retaining screws (3).
3. Disconnect the electrical connector(s) (1).
4. Remove the speaker assembly (2) from the door frame (4).

### Installation Procedure

1. Connect the electrical connector(s) (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the speaker assembly (2) to the door frame (4).
3. Install the front speaker assembly to door frame attaching screws (3).

Tighten
Tighten the screws to 2 N·m (18 lb in).

4. Install the front door trim panel. Refer to Front Side Door Trim Panel Replacement.