For 1990-2009 cars

### Removal Procedure

1. Remove the oil pan. Refer to Oil Pan Replacement.
2. Remove the oil pan scraper bolts (1).
3. Remove the oil pan scraper (2).
4. Remove the oil suction pipe to oil pan retaining bolts (1).
5. Remove the oil suction pipe (2).

Important: The oil suction pipe seal (1) is a single use component and must be discarded whenever the oil suction pipe (2) is removed.

6. Remove the oil suction pipe seal (1) from the oil suction pipe (2).

Discard the oil suction pipe seal (1).

### Installation Procedure

1. Install a NEW oil suction pipe seal (1) onto the oil suction pipe (2).
2. Install the oil suction pipe (2).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the oil suction pipe to oil pan retaining bolts (1).

Tighten
Tighten the bolts to 10 N·m (89 lb in).

4. Install the oil pan scraper (2).
5. Install the oil pan scraper to oil pan retaining bolts (1).

Tighten
Tighten the oil pan scraper bolts to 10 N·m (89 lb in).

6. Install the oil pan. Refer to Oil Pan Replacement.