For 1990-2009 cars

### Removal Procedure

1. Detach the soft tonneau cover (1) from the vehicle (2).
2. Detach the soft tonneau cover (1) from the vehicle (2).
3. Detach the soft tonneau cover magnetic strip (1) from the front of the cargo area (2).
4. Remove the front bow assembly (1) by sliding to the front of the vehicle.
5. Rotate the front bow assembly (1) anticlockwise.
6. Lifting one side at a time remove the soft tonneau assembly (2) from the soft tonneau cover bracket.
7. Remove the soft tonneau cover support bows (1) from the support bow brackets (2).

#### Disassembly

1. Lay the soft tonneau cover on a suitable clean surface, top facing upwards.
2. Fold the soft tonneau cover by starting from the rear corner and folding it to the opposite front corner.
3. Fold the soft tonneau cover from the rear corner and folding it to the opposite front corner.
4. Roll up the soft tonneau cover by starting from the rear most point of the cover.
5. Remove the soft tonneau cover from the front bow assembly (1) by sliding the locking strip (2) out of the front bow assembly (1).

### Installation Procedure

#### Assembly

1. Install the soft tonneau cover to the front bow assembly (1) by sliding the locking strip (2) into the front bow assembly (1).
2. Install the front bow assembly (1) to the vehicle one side at a time, positioning into the soft tonneau cover bracket (2).
3. Rotate the front bow assembly (1) clockwise.
4. Install the front bow assembly (1) by sliding rearward of the vehicle.
5. Unravel the soft tonneau cover.
6. Attach the soft tonneau cover magnetic strip (1) to the front of the cargo area (2).
7. Install the soft tonneau cover support bows (1) to the support bow brackets (2).
8. Attach the soft tonneau cover (2) to the vehicle (1).