For 1990-2009 cars

Important: The output shaft retainer ring (661) can not be reused, it must be replaced.

1. Use snap ring pliers to remove the output shaft to retainer snap ring (661).

Important: The carrier assembly (662) can be a 4 or 5 pinion design depending on model.

2. Remove the input carrier assembly (662) and remove the thrust bearing assembly (663).
3. Remove the input internal gear (664) and the reaction carrier shaft assembly (666).
4. Remove the thrust washer (669) and the reaction sun shell (670).