For 1990-2009 cars

### Removal Procedure

Caution: Refer to Gasoline/Gasoline Vapors Caution in the Preface section.

Important: The fuel system hose/pipes are serviceable individually or as a complete fuel/brake bundle assembly, the following procedure is servicing the fuel hose/pipes individually.

1. Disconnect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Before you service any fuel system connection, relieve the fuel system pressure. Refer to the Fuel Pressure Relief .
3. Remove the exhaust and exhaust heat shields. Refer to Exhaust System Replacement
4. Remove the engine. Refer to Engine Replacement
5. Disconnect the fuel and EVAP lines at the fuel tank. Refer to Fuel Tank Replacement
6. Disconnect the fuel and evaporative emission (EVAP) lines at the engine compartment.
7. Remove the retaining bolts (1) and the retaining nuts (1) securing the rear stone guard.
8. Remove all the fuel line bracket pop rivets securing the fuel and EVAP pipes to the vehicle body.
9. Remove all the fuel line bracket pop rivets securing the fuel and EVAP pipes to the body tunnel.
10. Remove the fuel and EVAP lines from the vehicle.

### Installation Procedure

1. Install the fuel and EVAP lines to the vehicle.
2. Install all the fuel line bracket pop rivets securing the fuel and EVAP pipes to the body tunnel.
3. Install all the fuel line bracket pop rivets securing the fuel and EVAP pipes to the vehicle body.
4. Install the retaining bolts (1) and the retaining nuts (1) securing the rear stone guard.
5. Connect the fuel and evaporative emission (EVAP) lines at the engine compartment.
6. Connect the fuel and EVAP lines at the fuel tank. Refer to Fuel Tank Replacement .
7. Install the engine. Refer to Engine Replacement .
8. Install the exhaust and exhaust heat shields. Refer to Exhaust System Replacement .
9. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .