For 1990-2009 cars

#### Tools Required

• | J 37789-A Oil Pump Remover/Installer

• | J 39119 Oil Pump Remover/Installer Adapter

1. Remove all pump retaining bolts (2) and pump bolt seals (3).
2. Install J 39119 (4) over stator shaft until it locks under splines.
3. Install J 37789-A (1).
4. To prevent slipping, securely fasten the J 37789-A J 37789-A around the J 39119 by tightening the bolt (1) with a wrench.
5. Turn the T-handle on top of J 37789-A .
6. Lift the pump (4) out of the case.
7. Remove the fluid pump seal (5).
8. Remove the pump cover to case gasket (6).