For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection.

Important: The headliner can be easily damaged or discoloured. Use care when working in the area of the headliner.

2. Open the sun glasses storage compartment (1) to reveal the retaining screw (2).
3. Remove the dome lamp assembly to roof retaining screw (2).

Important: Grasp the dome lamp assembly (4) and pull downwards to remove the dome lamp assembly (4) from the headliner assembly (3).

4. Remove the dome lamp assembly (4) from the headliner assembly (3).
5. Disconnect the dome lamp assembly electrical connector (2).
6. Disconnect the Bluetooth microphone electrical connector (1) if fitted.

### Installation Procedure

1. Install the dome lamp assembly (3) to the vehicle.
2. Connect the bluetooth microphone connector (1) if fitted.
3. Connect the dome lamp assembly electrical connector (2).
4. Insert the two locating arms (1) into the headlining assembly (4).
5. Push the dome lamp assembly (5) up into the headlining assembly (4).
6. Install the dome lamp assembly to roof retaining screw (3).

Tighten
Tighten the screw to 2 N·m (18 lb in).

7. Close the sun glasses storage compartment (2).
8. Connect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection.