For 1990-2009 cars

#### Tools Required

• | J 23327-1 Forward Clutch Spring Compressor (Bridge)

• | J 34627 J 34627 Snap Ring Remover and Installer

1. Install the transmission (low and reverse clutch outer, center, inner) seals (696) on the low and reverse clutch piston (695).
2. Lubricate the seals with assembly lubricant J 36850 or an equivalent.
3. Install the low and reverse clutch piston (695) into the case. The notch in the piston must be aligned with the parking brake pawl window, in the case.
4. Install the low and reverse clutch spring assembly (694).

4.1. | Using the J 23327-1 , compress the low and reverse clutch spring assembly (694).

4.2. | Using J 36850 install the low and reverse clutch retainer ring (693).