For 1990-2009 cars

### Removal Procedure

1. Remove the left side engine mount. Refer to Engine Mount Replacement - Left Side.
2. Remove the left side engine mount bracket to cylinder block retaining bolts (1).
3. Remove the left side engine mount bracket (2).

### Installation Procedure

1. Install the left side engine mount bracket (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the left side engine mount bracket to cylinder block retaining bolts (1).

Tighten
Tighten the bolt to 50 N·m (37 lb ft).

3. Install the left side engine mount. Refer to Engine Mount Replacement - Left Side.