For 1990-2009 cars

### Removal Procedure

1. Remove the cargo liner. Refer to Cargo Box Liner Replacement .

Important: Remove the cargo liner seal (1) starting from the outer edges of the cargo liner.

2. Remove the cargo liner seal (1) from the cargo liner (2).

### Installation Procedure

Important: When installing the cargo liner seal, start by attaching both ends of the seal and work your way towards the centre of the seal, making sure to attach the seal evenly from both ends.

Important: Make sure that the cargo liner seal is positioned correctly onto the cargo liner. Check the cargo liner and cargo liner seal are mated correctly. Failure to do so will result in incorrect installation of the cargo liner seal.

1. Install the cargo liner seal (1) to the cargo liner (2).
2. Install the cargo liner. Refer to Cargo Box Liner Replacement .