For 1990-2009 cars

1. Position the shift lever in PARK.
2. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

Notice: Refer to Fastener Notice in the Preface section.

3. Loosen the shift control linkage adjustment bolt to allow the adjuster (1) to slide freely.
4. Hold the selector lever on the transmission against the rear stop to eliminate any play.

Tighten
Tighten the shift control linkage adjustment nut to 9 N·m (80 lb. in).

5. Lower the vehicle.
6. Check the operation of the starting system with the shift lever in each position. The engine should only crank when the lever is in the PARK or NEUTRAL position.