For 1990-2009 cars

### Removal Procedure

1. Turn the ignition OFF.

Important: Do not disconnect the power steering fluid lines/hoses from the reservoir.

2. Remove the power steering fluid reservoir bolts and reposition the power steering fluid reservoir in order to provide access. Refer to Power Steering Fluid Reservoir Replacement .
3. Remove the camshaft position (CMP) sensor electrical connector (1) from the CMP sensor (2).
4. Remove the the CMP sensor to engine front cover retaining bolt (1).
5. Remove the CMP sensor (2) from the engine front cover.

### Installation Procedure

1. Install the CMP sensor (2) to the engine front cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the CMP sensor to engine front cover retaining bolt (1).

Tighten
Tighten the bolt to 10 N·m (89 lb in).

3. Install the CMP sensor electrical connector (1) to the CMP sensor (2).
4. Install the power steering fluid reservoir. Refer to Power Steering Fluid Reservoir Replacement .