For 1990-2009 cars

## Blower Motor Replacement RHD

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Remove the glove box assembly. Refer to Instrument Panel Compartment Replacement .
2. Remove the left floor air outlet duct. Refer to Floor Air Outlet Duct Replacement - Left Side .
3. Disconnect the blower motor electrical connector (1).
4. Remove the blower motor to blower assembly retaining screws (1).
5. Remove the blower motor (2) from the blower assembly (1).

### Installation Procedure

1. Install the blower motor (2) to the blower assembly (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the blower motor to blower assembly retaining screws (1).

Tighten
Tighten the screws to 2 N·m(18lb in).

3. Connect the blower motor electrical connector (1).
4. Install the left floor air outlet duct. Refer to Floor Air Outlet Duct Replacement - Left Side .
5. Install the glove box assembly. Refer to Instrument Panel Compartment Replacement .