For 1990-2009 cars

Application | Specification
--- | ---
Metric | English
Assist Handle Retaining Screws | 2 N·m | 18 lb in
Body Hinge Pillar Trim Retaining Torx screw | 2 N·m | 18 lb in
Cargo Area Rear Trim Panel Retaining Hooks | 2 N·m | 18 lb in
Centre Pillar Upper Trim Panel Torx Screw | 2 N·m | 18 lb in
Centre Sill Trim Panel Retaining Torx Screw | 2 N·m | 18 lb in
Child Restraint Anchor Retaining Bolt | 22 N·m | 16 lb ft
Quarter Lower Trim Panel Retaining Torx Screw | 2 N·m | 18 lb in
Rear Quarter Upper Lower Section Retaining Torx Screw (WM Only) | 2 N·m | 18 lb in
Rear Quarter Upper Retaining Torx Screw (WM Only) | 2 N·m | 18 lb in
Rear Quarter Upper Trim Panel Retaining Screw | 2 N·m | 18 lb in
Rear Sill Panel Trim Retaining Torx Screw | 2 N·m | 18 lb in
Sunshade Assembly Retaining Torx Screws | 2 N·m | 18 lb in
Windshield Garnish Moulding Retaining Torx Screw | 2 N·m | 18 lb in