For 1990-2009 cars

### Removal Procedure

1. Partially detach the weatherstrip. Refer to Front Door Opening Weatherstrip Replacement.
2. Grasp both sides at the top of the centre pillar lower trim panel (3) and pull away from the door opening, disengaging the centre pillar lower trim panel trim retaining clips (2).
3. Remove the centre pillar lower trim panel (3) from the lower sill trim panel retaining clips (1).

### Installation Procedure

1. Install the top edge of the centre pillar lower trim panel (3) into the upper centre pillar trim panel trim lower retaining clips (2)
2. Firmly push the centre of the lower trim panel (3) locating the lower trim panel retaining clips into the sheet metal.
3. Firmly push in the bottom edge of the centre pillar lower trim panel (3) into the lower sill trim panel (1).
4. Attach the weatherstrip. Refer to Front Door Opening Weatherstrip Replacement.