For 1990-2009 cars

## Headlamp Switch Replacement RHD

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove headlamp switch (1) from I/P trim pad by gently prizing the switch assembly from the IP crashpad.
3. Disconnect the headlamp switch electrical connector.
4. Remove the headlamp switch.

### Installation Procedure

1. Connect the headlamp switch electrical connector.
2. Install the headlamp switch (1) to the I/P trim pad.
3. Connect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection.
4. Check all vehicle lights for correct operation.