For 1990-2009 cars

## Drive Belt Tensioner Installation With Air Condictioning

1. Install the drive belt tensioner (2) to the engine front cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the drive belt tensioner to engine front cover retaining bolts (1).

Tighten
Tighten the bolts to 22 N·m (16 lb ft).

## Drive Belt Tensioner Installation Without Air Condictioning

1. Install the drive belt tensioner (1) to the engine front cover.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the drive belt tensioner to engine front cover retaining bolts (2).

Tighten
Tighten the bolts to 50 N·m (37 lb ft).