For 1990-2009 cars

1. Remove the valley cover retaining bolts (1).
2. Remove the valley cover (2).

Important: The valley cover gasket (3) is a single use only component and must be replaced whenever the valley cover gasket (3) is removed from the engine.

3. Remove the valley cover gasket (3).

Discard the valley cover gasket (3).

4. Remove the oil pressure sensor (1) and washer (2), as required.