For 1990-2009 cars

#### Tools Required

• | J 23327-1 Forward Clutch Spring Compressor (Bridge)

• | J-34627 Snap Ring Remover and Installer

• | J-42628 Disc

1. Install the J 23327-1 and the J-42628 .
2. Tighten the J 23327-1 .
3. Remove the low and reverse clutch retainer ring (693) using the J-34627 .
4. Remove the low and reverse clutch spring assembly (694).
5. Blow compressed air into the case passage to remove the low and reverse clutch piston (695).

• | (1) LO Feed Passage

• | (2) REV Feed Passage