For 1990-2009 cars

Callout | Component Name
--- | ---

#### Preliminary Procedures

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the transmission fluid pan and filter. Refer to Automatic Transmission Fluid, Fluid Pan and/or Filter Replacement .

1 | Manual Shift Shaft Position Switch Assembly Electrical Connector Tip

• | Release the connector lock before disconnecting. Engage the connector lock after connecting.

• | The wiring harness clip near the connector does not need to be replaced if broken or missing. The clip is used during manufacturing to keep the wire harness clear during an automated bolt installation process. If the clip is damaged, simply remove and discard.

2 | Manual Shift Shaft Position Switch Assembly Bolt Notice: Refer to Fastener Notice in the Preface section. Tighten 8 N·m (71 lb in)
3 | Manual Shift Shaft Position Switch Assembly

#### Procedure

Align the switch activator slide with the manual valve link.