For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Disconnect the reverse lamp switch electrical connector (3).
3. Using a suitable tool remove the reverse lamp switch (2) from the transmission (1).

### Installation Procedure

1. Apply a suitable pipe sealant with Teflon® to the threads of the backup lamp switch (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the backup lamp switch (2) to the transmission (1).

Tighten
Tighten the switch to 27 N·m (20 lb ft).

3. Connect the reverse lamp switch electrical connector (3).
4. Lower the vehicle.