For 1990-2009 cars

#### Tools Required

J 28410 Gasket Remover

### Cleaning Procedure

1. Remove any RTV sealant (1) from the engine front cover using J 28410 .
2. Clean out debris from the bolt holes.
3. Clean the engine front cover (1) in solvent.

Caution: Refer to Safety Glasses Caution in the Preface section.

4. Dry the engine front cover (1) with compressed air.

### Inspection Procedure

1. Inspect the exterior of the engine front cover for the following conditions:

• | Damage to the water pump bolt hole threads (7).

• | Gouges or damage to the water pump sealing surfaces (6).

• | Damage to the crankshaft front oil seal bore (5).

• | Damage to the camshaft position actuator solenoid seal bores (1).

• | Damage to the engine front cover bolt holes (2).

• | Damage and/or corrosion to the engine coolant passage (3).

• | Dents or damage to the exterior (4).

2. Inspect the interior of the engine front cover for the following conditions:

• | Gouges or damage to the engine front cover sealing surfaces to the cylinder block (7), oil pan (5), and/or camshaft covers (2).

• | Damage and/or corrosion to the engine coolant passage .(6)

• | Damage to the crankshaft front oil seal bore.

• | Gouges or damage to the O-ring sealing areas.

• | Gouges or damage to the water pump seal area (3).

• | Loose or damaged deadener plates (4).

• | Damage to the engine front cover bolt holes (1).

3. Repair or replace the engine front cover as necessary.