For 1990-2009 cars

## General Specifications 3.6L Engine

### Clutch Specifications (3.6L Engine)

Component | Application | Specification
--- | --- | ---
Master Cylinder | Type Bore Size Nominal Stroke | Compensating Port 19.05 mm 30 mm
Clutch Actuating Cylinder | Type | Concentric cylinder with adaptor including bleed screw.
Clutch fluid | Type | DOT 4 or Super DOT 4
Clutch Driven Plate | Type Outside Diameter Inside Diameter Thickness of disc assembly with 7,300 N load | Single plate dry disc. 254 - mm 165 - 1.5 mm 9.6 - 0.2 mm
Clutch Pressure Plate | Type | Recessed, with a press steel cover plate and a bevelled diaphragm spring.
Clutch Throw-out Bearing | Type Lubrication | Ball Race. Sealed with grease for life.
Dual Mass Flywheel | Serviceability | Spring dampened internally; the transmission side is recessed to accommodate the clutch assembly. Rotational free play maximum, including length tolerances and heat setting losses. None. Starter motor ring gear is not replaceable and machining of the clutch facing surface is not permitted.
Transmission input shaft splines and clutch pedal bushes | Lubricant | NLGI No 2 lithum soap based EP grease with molybdenum disulphide, such as shell Retinax HDX2 grease, BP Energrease LMS-EP23 or equivalent.

## General Specifications 6.0L Engine

### Clutch Specifications (6.0L Engine)

Component | Desription | Specification
--- | --- | ---
Master Cylinder | Type Bore Size Nominal Stroke | Compensating Port 19.05 mm 30 mm
Clutch Actuating Cylinder | Type Bore size Stroke | Concentric hydraulic actuating cylinder with side bleed port. Equivalent diameter - 30.6 mm 9.5 mm
Clutch fluid | Type | DOT 4 or Super DOT 4
Clutch Driven Plate | Type Outside Diameter Inside Diameter Thickness of disc assembly with 10,000 N load | Single plate dry disc 297 - mm 198 - mm 8.7- 0.35 mm
Clutch Pressure Plate | Type | Self-adjusting with pressed steel cover plate and multi-fingered bevelled diaphragm spring.
Clutch Throw-out Bearing | Type Lubrication | Ball Race. Sealed with grease for life.
Actuating cylinder guide sleeve | Lubricant | NLGI No 2 lithium soap based EP grease with molybdenum disulphide, such as sheel Retinax HDX2 grease, BP Energrease LMS-EP23 or equivalent.