For 1990-2009 cars

### Removal Procedure

Caution: Refer to Vehicle Lifting Caution in the Preface section.

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Raise and suitably support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the VSS bolt (2).
3. Remove the VSS (1) from the rear extension housing.

### Installation Procedure

1. Install the VSS (1) to the rear extension housing.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the VSS bolt (2).

Tighten
Tighten the bolt to 8 N·m (71 lb in).

3. Lower the vehicle.