For 1990-2009 cars

### Removal Procedure

Important: The rearview mirror windshield boss (1) is not serviced separately and is part of the windshield assembly.

Important: Insert a suitable tool into the access hole (3) on the rearview mirror windshield boss (1) and carefully lever the rearview mirror (2) away from the rearview mirror windshield boss.

1. Detach the rearview mirror (2) from the rearview mirror windshield boss (1).
2. Remove the rearview mirror (2) from the vehicle.

### Installation Procedure

Important: Slide the rearview mirror (2) downwards on the rearview mirror windshield boss (1) until an audible click is heard

1. Install the rearview mirror (2) to the rearview mirror windshield boss (1).
2. Make sure the rearview mirror (2) operates correctly.