For 1990-2009 cars

Callout | Component Name
--- | ---
Notice: Refer to Fastener Notice in the Preface section. Fastener Tightening Specifications: Refer to Fastener Tightening Specifications .
1 | Fluid Pump Cover Assembly
2 | Fluid Pump Cover Bolts M6 x 40 (Quantity: 13) Tip Hand tighten only.
3 | Alignment Tool and Bolt Tip

1. Center the J 46664 around the fluid pump cover assembly in the 9 o'clock position and tighten the alignment bolt.
2. Tighten the fluid pump cover bolts in the sequence shown.

Tighten
11 N·m (97 lb. in)

#### Special Tool

J 46664 Pump Cover Alignment Tool

4 | NEW 1-2-3-4 and 3-5 Reverse Clutch Housing Thrust Washer