For 1990-2009 cars

### Removal Procedure - Up to 17 Sept 2007

1. Disable the SIR system. Refer to SIR Disabling and Enabling .

Caution: Refer to Battery Disconnect Caution in the Preface section.

2. Disconnect the battery ground cable from the battery. Refer to Battery Negative Cable Disconnection and Connection .
3. Remove the instrument panel lower trim panel assembly. Refer to Instrument Panel Insulator Panel Replacement - Right Side .
4. Remove the instrument panel lower trim panel retainer. Refer to Instrument Panel Retainer Replacement .
5. Disconnect the clutch position switch electrical connector (1).

Important: Rotate the clutch position switch (2) clockwise a 1/4 turn, then pull to release from the clutch bracket (3).

6. Remove the clutch position switch (2).

### Installation Procedure - Up to 17 Sept 2007

Important: Rotate the clutch position switch (2) a 1/4 of a turn anti-clockwise to lock it into the clutch bracket (3).

1. Install the clutch position switch (2).
2. Connect the clutch position switch electrical connector (1).
3. Install the instrument panel lower trim panel retainer. Refer to Instrument Panel Retainer Replacement .
4. Install the instrument panel lower trim panel assembly. Refer to Instrument Panel Insulator Panel Replacement - Right Side .
5. Enable the SIR. Refer to SIR Disabling and Enabling .
6. Connect the battery ground cable to the battery. Refer to Battery Negative Cable Disconnection and Connection .
7. Road test vehicle for correct clutch operation.

### Removal Procedure - From 17 Sept 2007

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery ground cable from the battery. Refer to Battery Negative Cable Disconnection and Connection .
2. Disable the SIR system. Refer to SIR Disabling and Enabling .
3. Remove the instrument panel lower trim panel assembly. Refer to Instrument Panel Insulator Panel Replacement - Right Side .
4. Remove the instrument panel lower trim panel retainer. Refer to Instrument Panel Retainer Replacement .
5. Remove the clutch pedal assembly. Refer to Clutch Pedal Replacement .
6. Disconnect the clutch pedal position sensor electrical connector (1).
7. Remove the clutch pedal assembly to clutch pedal position sensor retaining bolt (2).
8. Remove the clutch pedal position sensor (3).

### Installation Procedure - From 17 Sept 2007

Important: Clutch pedal pin is located between the clutch pedal position sensor (3).

1. Install the clutch pedal position sensor (3).
2. Install the clutch pedal assembly to clutch pedal position sensor retaining bolt (2).

Tighten
Tighten the bolt to 13 N·m (115 lb in).

3. Connect the clutch pedal position sensor electrical connector (1).
4. Install the clutch pedal assembly. Refer to Clutch Pedal Replacement .
5. Install the instrument panel lower trim panel retainer. Refer to Instrument Panel Retainer Replacement .
6. Install the instrument panel lower trim panel assembly. Refer to Instrument Panel Insulator Panel Replacement - Right Side .
7. Enable the SIR. Refer to SIR Disabling and Enabling .
8. Connect the negative battery cable to the battery. Refer to Battery Negative Cable Disconnection and Connection .
9. Road test vehicle for correct operation.