For 1990-2009 cars

### Removal Procedure

#### Tools Required

• | J 25019 Bushing Service Set

• | J 34196-B Transmission Bushing Service Set

• | J 7004-A Universal Remover

• | J 8092 Universal Driver Handle - 3/4 in - 10

1. Inspect the reverse input clutch housing and drum assembly for the following conditions:

• | Damaged or worn bushings

• | Surface finish on the hub and outer housing - check band surface for flatness

• | Leak at the weld

• | Heat distortion

• | Rolled or distorted retaining ring groove

2. Using the J 25019-16 with the J 7004-A , remove the reverse input clutch front bushing (603).
3. Using the J 25019-4 with the J 8092 , remove the reverse input clutch rear bushing (606).

### Installation Procedure

1. Using the J 25019-9 with the J 8092 , install a reverse input clutch front bushing (603).
2. Using the J 34196-3 which is part of kit J 34196-B with the J 8092 , install a reverse input clutch rear bushing 606).