For 1990-2009 cars

## Front Fog Lamp Replacement Except HSV Maloo

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the air deflector from the front end of the vehicle. Refer to Front Air Deflector Replacement.
3. Disconnect the electrical connector (3) from the fog lamp assembly.
4. Remove the fasteners (1) that secure the front fog lamp assembly (2) to the front fascia.
5. Remove the front fog lamp assembly from the vehicle.

### Installation Procedure

Important: Do not handle the quartz envelope of the headlight bulb. Wipe the quartz envelope immediately with methylated spirits if it is touched accidentally or the performance of the bulb will deteriorate.

1. Install the front fog lamp assembly (2) to the front facia assembly.

Notice: Refer to Fastener Notice in the Preface section.

2. Install and tighten the retaining screws to secure the front fog lamp assembly to the front fascia.

Tighten
Tighten the retaining screws to 2.0 N·m (18 lb in).

3. Connect the electrical connector (3) to the fog lamp assembly.
4. Install the air deflector to the front end of the vehicle. Refer to Front Air Deflector Replacement.

Caution: Refer to Battery Disconnect Caution in the Preface section.

5. Connect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection.
6. Adjust the fog lamps. Refer to Fog Lamp Aiming.

## Front Fog Lamp Replacement HSV Maloo

### Removal Procedure - Type B

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the front air deflector. Refer to Front Air Deflector Replacement .
3. Disconnect the front fog lamp electrical connector (1).
4. Remove the front lamp assembly to fascia retaining screws (1).
5. Remove the front fog lamp adjustment screw (2) and spring (1).
6. Remove the front fog lamp to bracket retaining bolts (4).
7. Remove the front fog lamp (3) from the vehicle.

### Installation Procedure - Type B

1. Position the front fog lamp to the vehicle.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front fog lamp to bracket retaining bolts (4).

Tighten
Tighten the bolts to 2.0 Nm (18 lb in).

3. Install the front fog lamp adjustment screw (2) and spring (1).
4. Install the front lamp assembly to fascia retaining screws (1).

Tighten
Tighten the screws to 2.0 Nm (18 lb in).

5. Connect the front fog lamp electrical connector (1).
6. Install the front air deflector. Refer to Front Air Deflector Replacement .
7. Adjust the fog lamps. Refer to Fog Lamp Aiming .
8. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection .

### Removal Procedure - Type C

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection .
2. Remove the front air deflector. Refer to Front Air Deflector Replacement .
3. Cut and discard the cable tie (3).
4. Disconnect the front fog lamp electrical connector (2).
5. Remove the front fog lamp to fascia retaining screws (4).
6. Remove the front fog lamp assembly (1) from the vehicle.
7. Remove the front fog lamp to bracket retaining bolts (2).
8. Remove the front fog lamp (1).

### Installation Procedure - Type C

1. Position the front fog lamp (1) to the retaining bracket.

Notice: Refer to Fastener Notice in the Preface section.

2. Install the front fog lamp to bracket retaining bolts (2).

Tighten
Tighten the bolts to 2.0 Nm (18 lb in).

3. Install the front fog lamp assembly (1) and the front fog lamp assembly to fascia retaining screws (4).

Tighten
Tighten the screws to 2.0 Nm (18 lb in).

4. Connect the front fog lamp electrical connector (2).
5. Install a NEW cable tie (3).
6. Install the front air deflector. Refer to Front Air Deflector Replacement .
7. Adjust the fog lamps. Refer to Fog Lamp Aiming .
8. Connect the battery negative cable. Refer to Battery Negative Cable Disconnection and Connection .