For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.
2. Remove the rear wheels. Refer to Tire and Wheel Removal and Installation.
3. Remove the rear mud flap to rear fascia retaining screws (2).
4. Remove the rear mud flap (3) from the rear fascia (1).

### Installation Procedure

1. Position the rear mud flap (3) to the rear fascia (1).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the rear mud flap to rear fascia retaining screws (2).

Tighten
Tighten the screws to 4 N·m (35 lb in).

3. Install the rear wheels. Refer to Tire and Wheel Removal and Installation.
4. Lower the vehicle.