For 1990-2009 cars

Application | Specifications
--- | ---
Metric | English
Accelerator Pedal Position (APP) Sensor Assembly Retaining Bolts | 20 N·m | 15 lb ft
Air Cleaner Lower Housing Retaining Bolts | 10 N·m | 89 lb in
Camshaft Position (CMP) Sensor Retaining Bolt | 25 N·m | 18 lb ft
Crankshaft Position (CKP) Sensor Retaining Bolt | 25 N·m | 18 lb ft
Engine Coolant Temperature (ECT) Sensor | 20 N·m | 15 lb ft
Evaporative Emissions (EVAP) Canister Retaining Bolts | 6 N·m | 53 lb in
Fuel Filler Hose Clamps | 4 N·m | 35 lb in
Fuel Pipe Stone Guard Retaining Nuts | 5 N·m | 44 lb in
Fuel Rail Retaining Bolts | 10 N·m | 89 lb in
Fuel Tank Strap Upper Retaining Bolts | 20 N·m | 15 lb ft
Heated Oxygen Sensor (HO2S) | 41 N·m | 30 lb ft
Ignition Coil to Ignition Plate Assembly Retaining Bolts | 12 N·m | 106 lb in
Knock Sensor (KS) Retaining Bolt | 20 N·m | 15 lb ft
Spark Plug New Cylinder Head | 20 N·m | 15 lb ft
Spark Plug Old Cylinder Head | 15 N·m | 11 lb ft
Throttle Body Retaining Bolts | 12 N·m | 106 lb in
Fuel Rail Ground Strap To Intake Manifold Retaining Bolts | 10 N·m | 89 lb in
Air Cleaner Intake Duct to Throttle Body Retaining Clamp | 4 N·m | 35 lb in
Ignition Coil To Rocker Cover Retaining Blots | 12 N·m | 106 lb in
Fuel Filler Pipe to Chassis Retaining Bolts | 9 N·m | 80 lb in
Rear Subframe to Chassis Retaining Bolts
First Pass: | 65 N·m | 48 lb ft
Final Pass: | 125 Degrees
Intake Air Temperature/Mass Air Flow (AT/ MAF) to Air Intake Duct Retaining Clamp | 2 N·m | 18 lb in
Intake Air Temperature/Mass Air Flow (AT/ MAF) to Upper Air Cleaner Body Retaining Clamp | 2 N·m | 18 lb in