For 1990-2009 cars

### Removal Procedure

Important: Protect the paint and body work with tape or a clean cloth. Failure to do so may result in damage to the paint work.

Important: Apply heat to the body side emblem (1) using a suitable heat gun to reduce the adhesion to the body side (2).

Important: Using a suitable tool, carefully prise the body side emblem (1) from the body side (2). Take care not to damage the paint work.

1. Remove the body side emblem (1) from the body side (2).

Important: Clean the surface with a suitable cleaning solution and a lint free cloth to remove any remaining adhesive from the body side (2).

2. Remove any remaining adhesive from the body side (2).

### Installation Procedure

Important: The broken line (2) represents the HN2021 or equivalent polyethylene double sided tape. The image should only be used for reference.

Important: If reusing the body side emblem (1), clean the body side emblem (1) with a suitable cleaning solution using a lint free cloth.

Important: Do not allow the HN2021 or equivalent polyethylene double sided tape (2) to come in contact with any dirt or foreign matter.

1. Apply NEW HN2021 or equivalent polyethylene double sided tape (2) to the back of the body side emblem (1).
2. Trim back the HN2021 or equivalent polyethylene double sided tape (2) to the inner edge of the body side emblem (1).
3. Peel the backing from the HN2021 or equivalent polyethylene double sided tape (2).

Important: Firmly press the body side emblem (1) for 30 seconds to ensure correct adhesion.

4. Apply the body side emblem (1) to the body side (2). Refer to Graphics/Decals/Emblems for measurement specifications.