For 1990-2009 cars

## Clutch Vibration RHD

#### Clutch Vibration

Cause | Action
--- | ---
DEFINITION: Vibration from the clutch components during disengagement or engagement. Review the Symptoms - Clutch .
Excessive driveline torsional activity | Review the Clutch Vibration
Clutch incorrectly installed | Remove the clutch and install it correctly. Refer to Clutch Assembly Replacement .
Clutch pilot bearing worn or damaged - 6.0L |

1. Replace the clutch pilot bearing. Refer to Clutch Pilot Bearing Replacement for 6.0L engine.
2. Inspect the transmission input shaft pilot bearing journal for wear or damage.
3. Replace the transmission input shaft if the splines are excessively worn. Refer to Transmission Disassemble for Aisin AY6 or Transmission Disassemble for Tremec 6 speed.

Transmission input splines worn or damaged |

1. Inspect the clutch driven plate to input splines for wear or damage.
2. Replace the transmission input shaft if the splines are excessively worn. Refer to Transmission Disassemble for Aisin AY6 or Transmission Disassemble for Tremec 6 speed.

Clutch driven plate facings damaged | Replace the clutch assembly. Refer to Clutch Assembly Replacement .
Flywheel housing to clutch housing excessively misaligned | Replace the faulty clutch housing or transmission front case. Refer to Transmission Disassemble for Aisin AY6 or Transmission Disassemble for Tremec 6 speed .
Clutch out of balance | Replace the clutch assembly. Clutch Assembly Replacement .