For 1990-2009 cars

#### Tools Required

J 21426 Rear Seal Installer

1. Using the J 21426 , install an output shaft sleeve (690) and an output shaft seal (691).

Do not push the sleeve past the machined surface on the output shaft.

2. Install the case extension to case seal (30) and the case extension (31).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the case extension to case retaining bolts (32).

Tighten
Tighten the retaining bolts to 45 N·m (33 lb ft).

4. Inspect the transmission speed sensor for the following conditions:

• | Cracks

• | Nicks

• | Damage

5. Install a new O-ring seal (37) on the internal transmission speed sensor (36).
6. Install the internal transmission speed sensor (36).
7. Install the speed sensor retaining bolt (35).

Tighten
Tighten the bolt to 12 N·m (9 lb ft).

Important: If installing a slip yoke type seal (34), position drain hole (1) to bottom of transmission within area shown.

8. Using the J 21426 , install the case extension oil seal assembly (34) (model dependent).