For 1990-2009 cars

### Tools Required

• | J 29658-D Fuel Pressure Gauge

• | AU-453 Fuel Pressure Test Hose Adapter

Caution: Gasoline or gasoline vapors are highly flammable. A fire could occur if an ignition source is present. Never drain or store gasoline or diesel fuel in an open container, due to the possibility of fire or explosion. Have a dry chemical (Class B) fire extinguisher nearby.

Caution: Relieve the fuel system pressure before servicing fuel system components in order to reduce the risk of fire and personal injury.

After relieving the system pressure, a small amount of fuel may be released when servicing the fuel lines or connections. In order to reduce the chance of personal injury, cover the regulator and the fuel line fittings with a shop towel before disconnecting. This will catch any fuel that may leak out. Place the towel in an approved container when the disconnection is complete.

Caution: Refer to Safety Glasses Caution in the Preface section.

1. Turn the ignition OFF.
2. Disconnect the negative battery cable in order to avoid possible fuel discharge if an accidental attempt is made to start the engine. Refer to Battery Negative Cable Disconnection and Connection .
3. Remove the fuel injector sight shield.
4. Connect the EN-47620 (1) fuel pressure test hose adapter to the fuel pressure connection. Wrap a shop towel around the fitting while connecting the J 29658-D (1) in order to avoid spillage.
5. Connect the J 29658-D (2) fuel pressure gauge to the EN-47620 (1). Wrap a shop towel around the fitting while connecting the gauge in order to avoid spillage.
6. Install the bleed hose into an approved container.
7. Open the valve in order to bleed the system pressure. Fuel connections are now safe for servicing.
8. Drain any fuel remaining in the gauge into an approved container.
9. Install the fuel injector sight shield.
10. Connect the negative battery cable. Refer to Battery Negative Cable Disconnection and Connection .