For 1990-2009 cars

### Removal Procedure

1. Remove the door trim panel. Refer to Front Side Door Trim Panel Replacement .
2. Remove the window inner belt sealing strip. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement .
3. Remove the lower part of the inner window weatherstrip (3) from the door (1).

Important: Pull the inner window weatherstrip (2) to detach the retainers.

4. Remove the inner window weatherstrip (2) from the door (1).

### Installation Procedure

Important: Locate the weatherstrip (2) at the datum located at the front first. Push the inner window weatherstrip (2) to attach the retainers.

1. Install the inner window weatherstrip (2) to the door (1).
2. Install the lower part of the inner window weatherstrip (3) to the door (1).
3. Install the window inner belt sealing strip. Refer to Front Side Door Window Belt Inner Sealing Strip Replacement .
4. Install the door trim panel. Refer to Front Side Door Trim Panel Replacement .