For 1990-2009 cars

### Removal Procedure

1. Remove the sunshade assembly. Refer to Sunshade Replacement.
2. Using a suitable screwdriver, release the retaining tabs (1) on the retainer (2).
3. Remove the retainer (2).

### Installation Procedure

1. Install the sunshade retainer (2) by inserting the retaining tabs (1) into the roof panel, listen for an audible click to confirm fitting.
2. Install the sunshade assembly. Refer to Sunshade Replacement.