For 1990-2009 cars

Checks | Causes
--- | ---
1-2-3-4 and 3-5-R Clutch Assembly (51) |

• | Inspect for damaged or worn 3-5-R clutch plates (402-404).

• | Inspect for damaged 3-5-R clutch piston (421), apply ring (405), and spring (420).

• | Inspect for cut, worn, or damaged 3-5-R clutch piston dam O-ring seal (418), inner seal (419), and outer seal (422).

• | Inspect for improper selective 3-5-R clutch backing plate retaining ring (400).

• | Inspect for damaged 3-5-R clutch backing plate (401). Inspect for worn splines on the backing plate.