For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle .
2. Remove the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .

Important: The rear bumper fascia lower support to quarter panel retaining rivets (2) are single use parts and must be discarded after removal.

3. Drill out and remove the rear bumper fascia lower support to quarter panel retaining rivets (2).

Discard the rivets.

4. Remove the rear bumper fascia lower support (1) from the quarter panel (3).

### Installation Procedure

1. Position the rear bumper fascia lower support (1) to the quarter panel (3).
2. Install NEW rear bumper fascia guide lower support to quarter panel retaining rivets (2).
3. Install the rear bumper fascia. Refer to Rear Bumper Fascia Replacement .
4. Lower the vehicle.