For 1990-2009 cars

## Fastener Tightening Specifications SWBRHD

Application | Specification
--- | ---
Metric | English
A/C

- Compressor Retaining Bolts

22 N·m

17 lb ft

- Compressor Bracket Retaining Bolts

58 N·m

43 lb ft

- Compressor Hose Assembly to Compressor Retaining Bolt

9 N·m

80 lb in

Alternator

- Alternator to Alternator Bracket Retaining Studs

18 N·m

13 lb ft

- Alternator to Alternator Bracket Stud Retaining Nuts

18 N·m

13 lb ft

- Alternator Bracket to Engine Block Retaining Bolts - Side-M10

58 N·m

43 lb ft

- Alternator Bracket to Engine Block Retaining Bolts - Front-M10

58 N·m

43 lb ft

- Alternator Bracket to Engine Block Retaining Bolts - Side-M8

23 N·m

17 lb ft

- Battery Cable to Alternator Retaining Nut

13 N·m

115 lb in

Camshaft Position Actuator

- Camshaft Position Actuator to Camshaft Retaining Bolt

58 N·m

43 lb ft

- Camshaft Position Actuator Solenoid Valve to Engine Front Cover Retaining Bolt

10 N·m

89 lb in

Camshaft Bearing Cap to Cylinder Head Retaining Bolts | 10 N·m | 89 lb in
Camshaft Cover to Cylinder Head Retaining Bolts | 10 N·m | 89 lb in
Camshaft Intermediate Drive Chain Idler to Cylinder Block Retaining Bolt | 58 N·m | 43 lb ft
Camshaft Position Sensor to Engine Front Cover Retaining Bolt | 10 N·m | 89 lb in
Connecting Rod Bolt

- First Pass

30 N·m

22 lb ft

- Second Pass - Counter Clockwise

Back Off to Zero

- Third Pass

25 N·m

18 lb ft

- Final Pass

110 Degrees

Coolant Inlet Pipe

- Radiator Outlet Pipe to Alternator Mounting Bracket Retaining Nut

22 N·m

16 lb ft

Coolant Outlet Housing to Intake Manifold Retaining Bolts | 10 N·m | 89 lb in
Crankshaft Balancer to Crankshaft Retaining Bolt

- First Pass

100 N·m

74 lb ft

- Final Pass

150 Degrees

Crankshaft Bearing Cap to Cylinder Block Retaining Bolts
Inner

- First Pass

20 N·m

15 lb ft

- Final Pass

80 degrees

Outer

- First Pass

15 N·m

10 lb ft

- Final Pass

110 Degrees

Side

- First Pass

30 N·m

22 lb ft

- Final Pass

60 Degrees

Crankshaft Rear Oil Seal Housing to Cylinder Block Retaining Bolts | 10 N·m | 89 lb in
Cylinder Head to Cylinder Block Retaining Bolts - M8

- First Pass

15 N·m

10 lb ft

- Final Pass

60 Degrees

Cylinder Head to Cylinder Block Retaining Bolts - M11

- First Pass

45 N·m

33 lb ft

- Second Pass

Counter Clockwise 120 degrees

- Third Pass

30 N·m

22 lb ft

- Final Pass

150 degrees

Cylinder Head Coolant Threaded Plugs | 45 N·m | 33 lb ft

- Drive Belt Idler Pulley to Accessory Drive Mounting Bracket Retaining Bolt

58 N·m

43 lb ft

- Drive Belt Tensioner to Engine Front Cover Retaining Bolts

22 N·m

16 lb ft

Pressure Plate to Flywheel Retaining Bolts |
First Pass | 15 N·m | 11 lb ft
Second Pass | 30 N·m | 22 lb ft
Third Pass | 90° Degrees
Engine Flywheel to Crankshaft Retaining Bolts

- First Pass

30 N·m

22 lb ft

- Final Pass

75 Degrees

Engine Driveplate to Crankshaft Retaining Bolts

- First Pass

30 N·m

22 lb ft

- Final Pass

45 Degrees

Engine Front Cover to Cylinder Block Retaining Bolts

- First Pass

20 N·m

15 lb ft

- Final Pass

60 Degrees

Engine Cover Mounting Bracket to Cylinder Head Retaining Bolt | 35 N·m | 26 lb ft
Engine Mount

- Engine Mount Bracket to Cylinder Block Retaining Bolts

50 N·m

37 lb ft

- Engine Mount to Engine Mount Bracket Retaining Nut

80 N·m

59 lb ft

- Engine Mount to Front Subframe Retaining Nuts

80 N·m

59 lb ft

Fuel Injector Harness Electrical Connector/EVAP Valve Mounting Bracket to Intake Manifold Retaining Bolt | 10 N·m | 89 lb in
Engine Wiring Harness Bracket

- Engine Wiring Harness Bracket to Cylinder Head Rear Retaining Bolts

40 N·m

30 lb ft

- Engine Wiring Harness Bracket to Cylinder Block Retaining Bolt

10 N·m

89 lb in

- Engine Wiring Harness Bracket to Right Bank Cylinder Head Retaining Bolt

10 N·m

89 lb in

Engine Wiring Harness Ground

- Engine Wiring Harness Ground to Left Bank Cylinder Head Retaining Bolt

10 N·m

89 lb in

- Engine Wiring Harness Ground to Right Bank Cylinder Head Front Retaining Bolt

10 N·m

89 lb in

- Engine Wiring Harness Ground to Right Bank Cylinder Head Rear Retaining Bolt

10 N·m

89 lb in

Exhaust Manifold

- Exhaust Manifold to Cylinder Head Retaining Bolts

20 N·m

15 lb ft

- Exhaust Manifold Heat Shield to Exhaust Manifold Retaining Bolts

10 N·m

89 lb in

Fuel Injector Rail to Lower Intake Manifold Retaining Bolts | 10 N·m | 89 lb in
Vehicle Body Ground Cable to Cylinder Head Retaining Bolt | 50 N·m | 37 lb ft
Heater Pipe Assembly to Thermostat Housing Retaining Bolts | 10 N·m | 89 lb in
Ignition Coil to Camshaft Cover Retaining Bolts | 10 N·m | 89 lb in
Intake Manifold

- Engine Cover Ball Stud

7 N·m

62 lb in

- Intake Manifold Runner Control (IMRC) Flap to Upper Intake Manifold Retaining Bolts

10 N·m

89 lb in

- Upper Intake Manifold-to-Cylinder Head Retaining Bolts - Long

23 N·m

17 lb ft

- Upper Intake Manifold-to-Cylinder Head Retaining Bolts - Short

23 N·m

17 lb ft

- Upper Intake Manifold-to-Lower Intake Manifold Retaining Bolts

23 N·m

17 lb ft

Oil Pan Drain Plug | 25 N·m | 18 lb ft
Oil Filter Cap | 25 N·m | 18 lb ft
Oil Filter Housing Adapter

- Oil Filter Adapter to Cylinder Head Retaining Bolt - M10

65 N·m

48 lb ft

- Oil Filter Adapter to Cylinder Block Retaining Bolts - M8

23 N·m

17 lb ft

Oil Gallery Plug | 31 N·m | 23 lb ft
Oil Jet to Cylinder Block Retaining Bolts | 10 N·m | 89 lb in
Oil Level Indicator Tube Bracket to Cylinder Head Retaining Bolt | 10 N·m | 89 lb in
Oil Level Sensor to Oil Pan Retaining Bolt | 20 N·m | 15 lb ft
Oil Pan

- Front Cover to Oil Pan Retaining Bolts

23 N·m

17 lb ft

- Oil Pan to Cylinder Block Retaining Bolts - M8

23 N·m

17 lb ft

- Oil Pan to Crankshaft Rear Oil Seal Housing Retaining Bolts - M6

10 N·m

89 lb in

- Transmission to Oil Pan Retaining Bolts

48 N·m

17 lb ft

- Oil Pan Baffle to Oil Pan Retaining Bolts

10 N·m

89 lb in

- Oil Pan Scraper to Oil Pan Retaining Bolts

10 N·m

89 lb in

Oil Pressure Sender | 20 N·m | 15 lb ft
Oil Pump

- Oil Pump to Cylinder Block Retaining Bolts

23 N·m

17 lb ft

- Oil Pump Cover to Oil Pump Housing Retaining Bolts

10 N·m

89 lb in

Oil Suction Pipe to Oil Pan Retaining Bolts | 10 N·m | 89 lb in
Power Steering Pump

- Power Steering Bracket to Cylinder Head Retaining Bolt

58 N·m

43 lb ft

- Power Steering Bracket to Engine Front Cover Retaining Bolt

58 N·m

43 lb ft

- Power Steering Bracket to Cylinder Block Retaining Bolt

58 N·m

43 lb ft

- Power Steering Pump to Power Steering Pump Bracket Retaining Bolts

27 N·m

22 lb ft

- Power Steering Fluid Reservoir Bracket to Engine Front Cover Retaining Bolts

9 N·m

80 lb in

Primary Camshaft Drive Chain

- Primary Camshaft Drive Chain Lower Guide to Oil Pump Retaining Bolts

13 N·m

115 lb in

- Primary Camshaft Drive Chain Tensioner to Cylinder Block Retaining Bolts

23 N·m

17 lb ft

- Primary Camshaft Drive Chain Upper Guide to Cylinder Block Retaining Bolts

23 N·m

17 lb ft

Secondary Camshaft Drive Chain

- Secondary Camshaft Drive Chain Guide to Cylinder Block Retaining Bolts

23 N·m

17 lb ft

- Secondary Camshaft Drive Chain Shoe to Cylinder Block Retaining Bolt

23 N·m

17 lb ft

- Secondary Camshaft Drive Chain Tensioner to Cylinder Block Retaining Bolts

- First Pass

5 N·m

44 lb in

- Final Pass

23 N·m

17 lb ft

Spark Plugs
Fit New Spark Plug | 20 N·m | 15 lb ft
Refit Existing Spark Plug | 18 N·m | 13 lb ft
Starter Motor

- Starter Motor to Cylinder Block Retaining Bolts

58 N·m

42 lb ft

- Battery Positive Cable to Starter Motor Terminal Retaining Nut

13 N·m

115 lb in

Thermostat Housing to Cylinder Block Retaining Bolts | 10 N·m | 89 lb in
Throttle Body Bolts to Upper Intake Manifold Retaining Bolts | 10 N·m | 89 lb in
Transmission

- Transmission Support to Body Retaining Bolts

58 N·m

43 lb ft

- Shift Selector Linkage Rod to Shift Selector Shaft Retaining Nut

9 N·m

84 lb in

Water Pump

- Water Pump to Engine Front Cover Retaining Bolts

10 N·m

89 lb in

- Water Pump Pulley to Water Pump Retaining Bolts

10 N·m

89 lb in