For 1990-2009 cars

### Removal Procedure

1. Remove the spark plugs in order to ease crankshaft/engine rotation. Refer to Spark Plug Replacement.
2. Remove the engine front cover. Refer to Engine Front Cover Replacement.
3. Remove the right bank secondary camshaft drive chain tensioner. Refer to Secondary Camshaft Drive Chain Tensioner Removal - Right Side.

### Installation Procedure

1. Install the right bank secondary camshaft drive chain tensioner. Refer to Secondary Camshaft Drive Chain Shoe Installation - Right Side.
2. Install the spark plugs. Refer to Spark Plug Replacement.
3. Install the engine front cover. Refer to Engine Front Cover Replacement.
4. Install the engine covers. Refer to Engine Cover Replacement.