For 1990-2009 cars

### Removal Procedure

1. Remove the right side engine mount. Refer to Engine Mount Replacement - Right Side .
2. Remove the right side engine mount bracket to cylinder block retaining bolts (1).
3. Remove the right side engine mount bracket (2).

### Installation Procedure

1. Install the right side engine mount bracket (2).

Notice: Refer to Fastener Notice in the Preface section.

2. Install the right side engine mount bracket to cylinder block retaining bolts (1).

Tighten
Tighten the bolts to 50 N·m (37 lb ft).

3. Install the right side engine mount. Refer to Engine Mount Replacement - Right Side .