For 1990-2009 cars

### Removal Procedure

Caution: Refer to Battery Disconnect Caution in the Preface section.

1. Disconnect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection.
2. Remove the front dome lamp assembly. Refer to Dome Lamp Replacement.
3. Twist the dome light bulb (1) assembly counter clockwise and remove from the dome lamp assembly.
4. Remove the dome light bulb (1) by gently pulling it from the socket (2).

### Installation Procedure

1. Install a new dome light bulb (1) to the dome light socket (2).
2. Install the dome light bulb (1) assembly, into the lamp assembly and twist clockwise to secure.
3. Install the front dome lamp assembly. Refer to Dome Lamp Replacement.
4. Connect the battery ground cable. Refer to Battery Negative Cable Disconnection and Connection.
5. Test the front dome lamp for correct operation.