For 1990-2009 cars

### Removal Procedure

Caution: Refer to Safety Glasses Caution in the Preface section.

Caution: Refer to Vehicle Lifting Caution in the Preface section.

1. Raise and support the vehicle. Refer to Lifting and Jacking the Vehicle.

Caution: Refer to General Repair Instructions in the Preface section.

2. Remove the stabiliser bar insulator bracket to subframe retaining bolts (4) on both sides of the stabiliser bar (1).
3. Remove the stabiliser bar insulator bracket (3) from the subframe on both sides of the stabiliser bar (1).
4. Remove the stabiliser bar insulator (2) from both sides of the stabiliser bar (1).
5. Inspect all parts for wear and damage.

### Installation Procedure

1. Install the stabiliser bar insulator (2) to both sides of the stabiliser bar (1).
2. Install the stabiliser bar insulator bracket (3) to the subframe on both sides of the stabiliser bar (1).

Notice: Refer to Fastener Notice in the Preface section.

3. Install the stabiliser bar insulator bracket to subframe retaining bolts (4) on both sides of the stabiliser bar (1).

Tighten
Tighten the bolts to 22 N·m (16 lb ft).

4. Remove the safety stands.
5. Lower the vehicle to the ground.